**Temperature Measurement System: Algorithm**

1. Read analogue value and store in *sensorvalue*
2. If data is requested serailly, jump to: 4
3. Else jump to: 1
4. Send *sensorvalue* serially
5. Jump to:1